**Installation MODBus Set GA5903**

**Function:** This wire set is a tool to make communication trough Modbus possible**.** The setcan be applied to all heaters quipped with an EBM 966 control board and enables a connection between the Modbus Interface and the heater.

**Installation:**

**Connection to the control board:**

* Insert the 4-pole plug of the cable supplied into terminal J16 of the control board.



**Connection to heater’s terminal support:**

* Screw the white connector supplied somewhere on the terminal support or let it hang loose.
* Attach the the sticker underneath the connector as illustrated in the picture.
* Connect the yellow wire to **A/+**
* Connect the white wire to **B/-**
* Connect the green wire to **PE (GND)**

